Pos. 0 Acoustic wall and ceiling panels

 Richter Acoustic-CompactPanel slotted with SC 400280.

Specifications:

front: Slotted with 4 mm (0.16”) groove, distance between grooves 28 mm (1.1”).

core: Acoustically tuned MDF core with acoustic drilling on the back surface.

back: Balancing backer with black acoustical fleece adhered to back..

*Finish option 1. Specifier to select preference.*

finish: front: Melamine/HPL surface. Manufacturer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Color/pattern: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

edges: ABS edgebanding to match selection at 0.4mm to 2mm in thickness.

back: Balancing backer for panel stability.

*Finish option 2. Specifier to select preference.*

finish: front: Grade A 0.5mm thick wood veneer

 Veneer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Veneer cut: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Veneer match: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Clear finished.

edges: Wood veneer to match selected species of face veneer. 0.6mm to 2mm in thickness. Clear finished.

back: 0,5mm balancing veneer for panel stability , clear primed finish and

 black acoustical fleece.

Formats:

 Width: 100mm (3.93”) up to 1550mm. (61”) Additional widths on request.

 Length: 304mm (11.97”) up to 4000mm (157.48”). Additional lengths on request.

 Thickness: 17mm (0.67”), 19mm (0.75”), 20mm (0.79”). Optional thicknesses on request.